MRB MATH LIBRARY

DOCUMENTATION

This library is intended for use in lower-cost, slower microcontrollers not dedicated for mathematical calculations (e.g. ATmega/Arduino, ARM Cortex M0 and M4, ESP, Raspberry Pi pico) to speed up floating point operations. It can also be used in DSP to reduce cycle time, wherever cycle time is very critical, but the accuracy of calculations is not so critical. The MRB\_MATH library will also significantly speed up the execution time of math calculations on microcontrollers without FPU or without hardware support for the default math.h library. An additional function not included in the math.h library is the function for calculating the RMS of a signal. This function is available in three variants: normal, fast and rapid.

In summary, this library allows faster calculations at the expense of lower precision and higher memory usage.

The documentation describes the functions contained in the MRB\_MATH library and compares them with their counterparts from the math.h library. Execution times and precision are compared. The results are summarized in graphs or tables. The possibility to parameterize each function is also described - the MRB\_MATH library makes it possible to increase the precision of a function at the cost of additional cycles or FLASH/RAM memory usage.

Functions included in the library

* **sin\_f**(float x) sinus from argument x
* **cos\_f**(float x) cosinus from argument x
* **fast\_invsqrt**(float x) fast inverse root square from argument x
* **fast\_sqrt**(float x) fast root square from argument x
* **RMS**(float x) root mean square function (with normal sqrt function)
* **fast\_RMS**(float x) fast root mean square function (with fast sqrt function)
* **rapid\_RMS**(float x) rapid root mean square fun. (approach without sqrt)
* **DFT**(float x) discrete Fourier transform

Execution speed overview

Table 1 Comparison of function execution time in terms of cycles on STM32 microcontroller with Cortex M-7 core

|  |  |  |
| --- | --- | --- |
| **Function / Library** | **<math.h>** | **“MRB\_MATH\_LIB.h”** |
| sinus | 762 cycles | 90 cycles |
| cosinus | 762 cycles | 92 cycles |
| sqrt | 674 cycles | 28 cycles |
| RMS | - | 694 cycles |
| fast RMS | - | 46 cycles |
| rapid RMS | - | 13 cycles |
| DFT | - |  |

Library created by Maciej Brzycki ------ February 2024

# Trigonometric functions

The sine and cosine functions in the MRB\_MATH library are based on the look up table, which will be stored in the microcontroller's flash memory when the program is uploaded. While the program is running, it permanently occupies space in RAM memory. User can define the size of memory usage with *LUTSIZE* parameter. When equal to 1 - look up table will take about 4kB of memory (1000 float values), when 2 – 8kB and when 4 – 16kB.

**Important note**: the range of the function's arguments is not as large as that of the **sin** function from the math.h library. The argument of the **sin\_f** function **should be** in range from the range -2π to 4π. For wider range of arguments **sin\_f** and **cos\_f** will work, but computing time will be longer.




Figure 1 LUT size choice

A screenshot of a computer


Description automatically generated

Figure 2 LUT view - beginning of the declaration





Figure 3 Use of trigonometric functions

A graph of a function

Description automatically generated

Figure 4 math.h sin(x) function and MRB\_MATH\_LIB.h sin\_f(x) comparison (LUTSIZE = 1)

A green graph with a white background

Description automatically generated

Figure 5 Absolute error between sin and sin\_f functions (LUTSIZE = 1)

A graph of a graph

Description automatically generated

Figure 6 cos and cos\_f comparison - zoom in

Table 2 Mean absolute difference between sin and sin\_f (or cos and cos\_f) with 1e-5 angle step.

|  |  |  |  |
| --- | --- | --- | --- |
| **LUTSIZE(n\*4kB)** | **1n** | **2n** | **4n** |
| **Mean Absolute error** | 0.000326 | 0.000163 | 0.000082 |

# Square root function

The fast square root function is based on inverse square root Quake’s algorithm. The Quake algorithm avoids directly calculating the square root. Instead, it uses a fast approximation, combined with Newton’s method for refinement. The key trick is in using bit-level manipulation of the floating-point number to produce a rough initial guess.

A computer screen with text and numbers

Description automatically generated

Figure 7 Quake algorithm

**Step-by-step Quake’s algorithm description:**

**Approximation using a "magic number":**

* The number *x* is first reinterpreted as an integer (using *\*(long int\*)&x*), which allows bit manipulation – e.g. float number *1.0f* would be reinterpreted as *1065353216*.
* This integer is then modified using a "magic constant" **0x5f3759df**, which was empirically determined. The expression *i = 0x5f3759df - (i >> 1)* performs the bit manipulation to get an initial approximation of .
* This step essentially tricks the floating-point representation into giving an initial estimate that’s close to the correct result.

**Convert the bits back to a float:**

* After the bit manipulation, the result is cast back into a floating-point value (using *\*(float\*)&i*), so now *y* is a rough approximation of ​.

**Refinement using Newton's method:**

The result is then refined with one iteration of Newton’s method to improve the approximation. This step reduces the error in the approximation. The formula used is:

After that, result of Quake’s algorithm is multiplied by input value, so division is avoided again (which increases execution speed a lot). Instead function does:

A computer screen with text

Description automatically generated with medium confidence

Figure 8 Inverse-Inverse square root

User can adjust the function by changing *SQRT\_ACCURACY* parameter. Increasing SQRT\_ACCURACY also increases linearly execution speed of the function. The relative error (relative to **sqrt** function from the math.h library) and the execution time of the function for a given parameter value are summarized below. The error was presented in relative form due to the very large range of values tested by the **fast\_sqrt** function.




Figure 9 Adjusting fast quare root accuracy - in default equal to 5

A graph of a function

Description automatically generated

Figure 10 sqrt from math.h and fast\_sqrt comparison

A graph with a line

Description automatically generated

Figure 11 Relative error [%] of fast\_sqrt function in comparison to sqrt function from math.h library

Table 3 Mean relative error of fast\_sqrt function with SQRT\_ACCURACY parameter change

|  |  |  |
| --- | --- | --- |
| **SQRT\_ACCURACY** | **Mean relative error** | **Function execution speed** |
| 2 | 1,6e-4 [%] | 17 cycles |
| 3 | 3,5e-6 [%] | 21 cycles |
| 5 | 2,3e-6 [%] | 26 cycles |
| 10 | 2,2e-6[%] | 44 cycles |
| 20 | 2,1e-6[%] | 90 cycles |

# Root mean square function

As is this one of the most commonly needed tools in digital signal processing, the root mean square function (RMS) has also been added to MRB\_MATH library. Three variants of the RMS function are included in this library: normal, fast and rapid. The normal variant is based on the sqrt function included in the math.h library. The fast variant is based on the fast\_sqrt function contained in the MATH\_MRB library. The rapid variant uses mathematical relationships assuming a perfectly sinusoidal waveform, so it does not use division or root operations. The accuracy of the various variants and their execution times for different signals is summarized below.

The user must set the parameters of the measured RMS signal in the preprocessor directives before using any of this functions (this must be done in the preprocessor, in order to avoid using the malloc() function to create a sample buffer). Important information is signal measuring frequency, base frequency for which RMS should be calculated and buffer size (should be counted as *measuring frequency divided by base frequency*). *RMS\_HANDLERS* corresponds to number of buffer arrays that are declared for this scope. Each signal should have different buffer. That means, e.g. for three phase system, there are three current measurements and three voltage measurements, so *RMS\_HANDLERS* should be equal to 6.

A screen shot of a computer

Description automatically generated

Figure 12 Setting parameters of RMS functions

A screen shot of a computer

Description automatically generated

Figure 13 Approach for use of RMS function with multiple occurrences

Table 4 Execution speed comparison for different RMS functions

|  |  |
| --- | --- |
| **Execution speed** | |
| **RMS** | 694 cycles |
| **fast\_RMS** | 46 cycles |
| **rapid\_RMS** | 13 cycles |

A graph with a green line and blue line

Description automatically generated

Figure 14 Comparison of transient state of normal RMS and rapid RMS for ideal sinusoidal signal

A graph showing a graph of a graph

Description automatically generated with medium confidence

Figure 15 Comparison for noisy signal with third harmonic injected

A graph with a line going up

Description automatically generated

Figure 16 Relative error of rapid\_RMS in comparison to normal RMS

# Discrete Fourier transform function

The last tool in the library is a discrete Fourier transform function designed for online computing on a microcontroller. Before using, user have to adjust preprocessor parameters: *DFT\_HANDLERS, SAMPLING\_FREQ,* *BASE\_FREQ, MAX\_HARMONIC* and *DFT\_RESULUTION*. Macro *MAX\_HARMONIC* corresponds with the highest frequency to which algorithm will count. The more harmonics we want to calculate, the longer computing will be needed. *DFT\_ RESULUTION* sets the difference between samples in **DFT** results. With accuracy equal to one, results are received with accuracy to one harmonic (results table will look like: h1, h2, h3 etc.). With accuracy equal to two results table will look like: h1, h1.5, h2 etc. Along with increasing resolution, the buffer array is getting bigger and computing time increases.

*DFT\_HANDLERS* corresponds to the number of buffer arrays that are declared for this scope. Each signal should have a different buffer. That means if user wants to make online DFT for 3 signals, for optimal memory usage, this parameter should be equal to 3. To store DFT results user also must declare array with proper length (at least half the buffer plus one).

A screen shot of a computer

Description automatically generated

Figure 17 Definition of DFT parameters

A computer code with text

Description automatically generated with medium confidence

Figure 18 Multiple occurrence of DFT function and result array definition

Execution speed of DFT function highly depends on buffer size (which is determined by the sampling frequency and resolution) and amount of harmonics which will be calculated. The **DFT** function called in program with a sampling frequency most of the time collects samples into a buffer and will perform calculations only after it is full. For a frequency of 50 Hz, the most costly actions for the processor will be performed every 20ms. After the first buffer is full, the buffer is cycled and the next calculation will be performed for a completely new set of samples.

Table 5 Exuction speed of DFT - comparison for different sampling and resolution parameters

|  |  |
| --- | --- |
| Buffer size | Execution speed |
| 100 (5kHz sampling, DFT resolution 1) |  |
| 200 (10kHz sampling, DFT resolution 1) |  |
| 800 (20kHz sampling, DFT resolution 2) |  |
| 20000 (40kHz sampling, DFT resolution 5) |  |

Figures 19 and 20 shows Fourier spectrums under various test conditions. Figure 19 shows Fourier spectrum of tested 50,5Hz sinusoidal signal contaminated with 2nd , 3rd , 5th and 7th harmonics. Test results were similar for all frequency sampling conditions.

Second figure presents difference in results between different resolutions. Signal for second test was additionally contaminated with non-integer harmonics (1.1n, 1.2n, 1.5n, 1.6n and 1.8n) every with an amplitude equal to 5% of 1st harmonic amplitude.

A graph with a line

Description automatically generated

Figure 19 Fourier spectrum - DFT test for non-ideal 50,5Hz sinusoidal signal and 2,3,5,7n harmonics

A graph of a graph

Description automatically generated

Figure 20 Fourier spectrum - DFT test for different DFT\_RESOLUTION parameters